{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["BoQ1","Macros"],"not_rendered":{"macros":1,"external_links":3,"defined_names":31},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"BoQ1","index":0,"n_rows":20,"n_cols":243,"rows_kept":20,"hidden":true,"merged":[[0,0,0,11],[3,0,3,54],[4,0,4,54],[5,0,5,54],[6,0,6,54],[7,1,7,54],[8,0,8,54],[19,2,19,54]],"flags":["formulas_cached_only"]}
["Item Rate BoQ"]
["BoQ_Ver3.0","Item Rate","Normal","INR Only","INR"]
["Select, Excess (+), Less (-)",null,"Less (-)"]
["Tender Inviting Authority: Superintending Engineer, EUDC-Technical, Noida"]
["Name of Work: DETAILS OF WORK AND QUANTITY AGAINST E-TENDER NO. 09/EUDC-T/2025-26/NOIDA (WORKS) FOR CARRYING OUT THE WORK OF LOCATING & PIN PONTING THE LT UNDER GROUND CABLE FAULT BY FAULT LOCATOR MACHINE AND REMOVAL OF FAULTS FOR PERIOD ONE YEAR (DATED 01.04.2026 TO 31.03.2027) UNDER EUDD-TECHNICAL, 11 & LT NETWORK - STADIUM / EXPRESSWAY / YEIDA, NOIDA IN THE JURIDICTION OF EUDC-TECHNICAL, NOIDA. (ALL TYPE LABOUR, MACHINE AND MATERIAL WILL BE PROVIDING BY THE CONTRACTOR AT HIS OWN COST ON TIME)."]
["Contract No: 0120-2970605"]
["The bidder quoted rate should be inclusive GST & all other taxes."]
["Name of the Bidder/ Bidding Firm / Company :"]
["(This BOQ template must not be modified/replaced by the bidder and the same should be uploaded after filling the relevent columns, else the bidder is liable to be rejected for this tender. Bidders are allowed to enter the Bidder Name and Values only)\nNote:- 1. In case the tenderer quotes impractical rates for the work / material and does not enter into a contract, action will be taken to confiscate the earnest money of the tenderer and blacklist the firm.\n2. Any type of NOC for the completion of following work will be received by the bidder itself only, Department will not be liable for these NOC.\n3- The bidder shall procure the jointing kits from Raychem/Denson/3M make, strictly in accordance with the GTP approved by PVVNL, Meerut. The bidder shall arrange for inspection/testing of the materials as per departmental rules S.E. (DQC) PVVNL Meerut through the Superintending Engineer. After testing, the materials will be handed over in a single lot to the engineer nominated by the Superintending Engineer.\n4- The jointing kit / work will have a warranty period of 12 months. If the jointing kit damaged during the warranty period, the contracting agency will replace the jointing kit (including fault location and rectification) free of charge."]
["NUMBER #","TEXT #","TEXT #","NUMBER #","TEXT #","NUMBER","NUMBER","TEXT","TEXT #","NUMBER #","TEXT#","TEXT #","NUMBER #","NUMBER","NUMBER","NUMBER","NUMBER","TEXT","TEXT","NUMBER","NUMBER","NUMBER","NUMBER","TEXT","TEXT","NUMBER","NUMBER","NUMBER","NUMBER","TEXT","TEXT","NUMBER","NUMBER","NUMBER","NUMBER","TEXT","TEXT","NUMBER","NUMBER","NUMBER","NUMBER","TEXT","TEXT","NUMBER","NUMBER","NUMBER #","NUMBER #","TEXT","TEXT","NUMBER #","NUMBER #","DATE","NUMBER #","NUMBER #","TEXT #"]
["Sl.\nNo.","Item Description","Item Code / Make","Quantity","Units","Estimated Rate in\nRs.      P",null,null,"Addition / Deduction","Addition / Deduction Values","Currency Convertion against each Item","Quoted Currency in INR / Other Currency","BASIC RATE In Figures To be entered by the Bidder with GST & all other taxes\nRs.      P\n","Excise Duty","VAT","Freight Charges ( Unloading & Stacking)","Any Other Taxes/Duties/Levies",null,null,"Other Taxes 2","IIIrd Party i.e DGS&D / RITES etc Inspection Charges @0.34%+Service Tax","Less for Cenvat Credit,if any respect of Supplies Under full Excise Duty Category ",{"$nulls":30},"TOTAL AMOUNT  With Taxes in\nRs.      P","TOTAL AMOUNT  With Taxes","TOTAL AMOUNT  With Taxes In Words"]
[1,2,3,3,4,6,7,8,9,10,11,12,5,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,42,43,44,45,46,47,48,49,50,51,52,6,54,7]
[{"v":1,"d":"1.00"},"Location and pin pointing of LT cable fault (exposing the same in the underground LT cable including digging of trench upto the depth of the cable, cutting the faulty cable and sealing of the faulty cable, high pressure cable) by Cable fault locator Machine mounted on a vehicle will be provided by the Contractor and Experinced Technicians, driver and helpers to operate the above machine will be provided by the contrator.",{"$nulls":236},1,"Construction of chamber for 100mm sluices valve","item1",10,"1 Nos"]
[1.01,"To locate the LT fault & digging of trench with the help road cutter/digging machine/tractor etc. (size of trench 3 m length & 1.5 m width) & Road restoration after rectification of fault to the same standard as on start of work or as per Authority norms.",null,800,"Nos",{"v":100,"d":"100.00"},null,null,"Excess(+)",1,"Full Conversion","INR",{"$nulls":40},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"INR Zero Only",{"$nulls":183},1.01,"Supplying, Conveying and fixing spls. Including eart","item1",123.223,"Nos"]
[1.02,"Providing LT Straight through with jointer per LT joint for filling. (LT 3.5x70/150/240/400 Sq.mm. straight through of Raychem/ 3M/ Denson make will be provided by the contractor).",null,700,"Nos",{"v":100,"d":"100.00"},null,null,"Excess(+)",1,"Full Conversion","INR",{"$nulls":40},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"INR Zero Only",{"$nulls":183},1.02,"Construction of chamber for 100mm sluice plates","item2",213,"Nos"]
[1.03,"Providing LT Outdoor / Indoor Jointing Kit with jointer per LT joint for filling. (LT 3.5x70/150/240/400185/240/300 Sq.mm. Outdoor / Indoor Jointing Kit of Raychem/ 3M/ Denson make will be provided by the contractor).",null,350,"Nos",{"v":100,"d":"100.00"},null,null,"Excess(+)",1,"Full Conversion","INR",{"$nulls":40},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"INR Zero Only",{"$nulls":183},1.02,"Construction of chamber for 100mm sluice plates","item2",213,"Nos"]
[1.04,"Replacement of LT damaged cable (approx 5 Mtrs. in each case for LT) (cable shall be provided by the department). Laying of cable in trench after making joint and filling of sand/brick/soil as per site requirement.","BI01010001010000000000000515BI0100001116",800,"Nos",{"v":100,"d":"100.00"},null,null,"Excess(+)",1,"Full Conversion","INR",{"$nulls":40},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"INR Zero Only",{"$nulls":183},1.02,"Construction of chamber for 100mm sluice plates","item2",213,"Nos"]
["Total in Figures",{"$nulls":51},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"INR Zero Only",{"$nulls":183},4,"Construction of chamber for 100mm sluice plates","item5",10,"Nos"]
["Quoted Rate in Figures",{"$nulls":3},"Select",{"$nulls":47},{"v":0,"d":"0.0000"},{"v":0,"d":"0.0000"}," Zero Only"]
["Quoted Rate in Words",null,"INR Zero Only"]

{"sheet":"Macros","index":1,"n_rows":6,"n_cols":5,"rows_kept":6,"merged":[[5,4,13,10]],"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[]
[{"$nulls":4},"Please Enable Macros to View BoQ information"]