{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["BoQ1","Macros"],"not_rendered":{"macros":1,"external_links":5,"defined_names":35,"comments":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"BoQ1","index":0,"n_rows":18,"n_cols":243,"rows_kept":18,"hidden":true,"merged":[[0,0,0,11],[3,0,3,54],[4,0,4,54],[5,0,5,54],[6,0,6,54],[8,0,8,54],[17,2,17,54]],"flags":["formulas_cached_only"]}
["Percentage BoQ"]
["BoQ_Ver3.0","Percentage","Normal","INR Only","INR"]
["Select, At Par, Excess (+), Less (-)",null,"IOCL"]
["Tender Inviting Authority: Executive Engineer, Kangsabati Canals Division No- I, Amlagora, Paschim Medinipur."]
["Name of Work: Supply of Empty Cement polythene Bags for Flood Precausionary Measure to the Ex-Zamindari Embankment at different places in Manoharpur -I & II G.P of Chandrakona-I Block under K.C. Division No-VII , Amlagora , Paschim Medinipur during the year 2023-24."]
["Contract No:  WBIW/EE/KCD-I/e-NIT- 02(e)/2023-24 [2nd Call of eNIT-  WBIW/EE/KCD-I/e-NIT- 01(e)/2023-24 for Sl-03, Sl-04, Sl- 05, Sl-06, Sl-07, Sl-08, Sl-09, Sl-10, Sl-11, Sl-14)  (Sl-02)"]
[" "]
["Name of the Bidder/ Bidding Firm / Company :"]
["PRICE SCHEDULE\n(This BOQ template must not be modified/replaced by the bidder and the same should be uploaded after filling the relevent columns, else the bidder is liable to be rejected for this tender. Bidders are allowed to enter the Bidder Name and Values only )"]
["NUMBER #","TEXT #","TEXT #","NUMBER #","TEXT #","NUMBER","NUMBER","TEXT","TEXT #","NUMBER #","TEXT#","TEXT #","NUMBER #","NUMBER","NUMBER","NUMBER","NUMBER","TEXT","TEXT","NUMBER","NUMBER","NUMBER","NUMBER","TEXT","TEXT","NUMBER","NUMBER","NUMBER","NUMBER","TEXT","TEXT","NUMBER","NUMBER","NUMBER","NUMBER","TEXT","TEXT","NUMBER","NUMBER","NUMBER","NUMBER","TEXT","TEXT","NUMBER","NUMBER","NUMBER #","NUMBER #","TEXT","TEXT","NUMBER #","NUMBER #","DATE","NUMBER #","NUMBER #","TEXT #"]
["Sl.\nNo.","Item Description","Item Code / Make","Quantity","Units","Estimated Rate in\nRs.      P",null,null,"Addition / Deduction","Addition / Deduction Values","Currency Convertion against each Item","Quoted Currency in INR / Other Currency","BASIC RATE In Figures To be entered by the Bidder \nRs.      P\n ","Excise Duty","VAT","Freight Charges ( Unloading & Stacking)","Any Other Taxes/Duties/Levies",null,null,"Other Taxes 2","IIIrd Party i.e DGS&D / RITES etc Inspection Charges @0.34%+Service Tax","Less for Cenvat Credit,if any respect of Supplies Under full Excise Duty Category ",{"$nulls":30},"TOTAL AMOUNT  Without Taxes in\nRs.      P","TOTAL AMOUNT  With Taxes","TOTAL AMOUNT \nIn Words"]
[1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,42,43,44,45,46,47,48,49,50,51,52,53,54,55]
[1,"Supplying to site empty cement polythene bags(capacity 50kg) in good condition including stacking,incedental charges etc.all complete (capacity 50 kg).",null,{"v":6000,"d":"6000.000"},"each",{"v":7.15,"d":"7.150"},null,null,"Excess(+)",1,"Full Conversion","INR",{"$nulls":40},{"v":42900,"d":"42900.000"},{"v":42900,"d":"42900.000"},"INR  Forty Two Thousand Nine Hundred    Only",{"$nulls":183},1.02,"Construction of chamber for 100mm sluice plates","item2",213,"Nos"]
[2,"Labour charges for filling empty cement gunny bag / polythene bag (capacity 50 kg) with all kind so fearth(wet or dry), sand or agreegates(stone / brick) and sewing as done incase of cement bags, (tying with a knot after filling will not be accepted),and stacking with in a lead of 30 metre as per direction of Engr-in-charge (cost is excluding the cost of any types of filling materials). NB:-Volume of earth/ sand filled bags should not be less than 0.028cum/ bag.",null,{"v":6000,"d":"6000.000"},"each",{"v":8.34,"d":"8.340"},null,null,"Excess(+)",1,"Full Conversion","INR",{"$nulls":40},{"v":50040,"d":"50040.000"},{"v":50040,"d":"50040.000"},"INR  Fifty Thousand  &Forty  Only"]
[3,"Dumping in position earth/ sand filled gunny /polybags (capacity 50 kg) within a lead of 30 metre inclusive of all lifts.",null,{"v":6000,"d":"6000.000"},"Meter",{"v":3.58,"d":"3.580"},null,null,"Excess(+)",1,"Full Conversion","INR",{"$nulls":40},{"v":21480,"d":"21480.000"},{"v":21480,"d":"21480.000"},"INR  Twenty One Thousand Four Hundred & Eighty  Only"]
["Total in Figures",{"$nulls":51},{"v":114420,"d":"114420.000"},{"v":114420,"d":"114420.000"},"INR  One Lakh Fourteen Thousand Four Hundred & Twenty  Only",{"$nulls":183},4,"Construction of chamber for 100mm sluice plates","item5",10,"Nos"]
["Quoted Rate in Figures",{"$nulls":3},"Select",{"$nulls":47},{"v":0,"d":"0.000"},{"v":0,"d":"0.000"},"INR Zero Only"]
["Quoted Rate in Words",null,"INR Zero Only"]

{"sheet":"Macros","index":1,"n_rows":6,"n_cols":5,"rows_kept":6,"merged":[[5,4,13,10]],"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[]
[{"$nulls":4},"Please Enable Macros to View BoQ information"]